| Prior to application installation: If you have never installed one of our 301/302 devices on your PC, you must first do so using the following procedure: 1.) BEFORE CONNECTING THE USB CABLE to your new 30x device get the correct installation files for your version of Windows at, "download page." There are versions there for Win2k/WinXP/WinVista/Win7/ (including 64-bit versions). Note that the installation for Win7 will also work for Win8 which hasn't yet been released as of the date of this writing (see update info at bottom). 2.) Follow the installation procedure outlined in "HowToApp.htm" found within the archives there. Application usage: 1.) If you are not an application developer, note that there are four files of interest to you within the UserApp.zip archive:
| RunFirst.bat LL_USB2k.EXE LL_USB.CFG LL_USB2k.DLL
Double-click the RunFirst.bat to run it. It will install the necessary support files in the Windows folder. 2.) Right-click the mouse on "LL_usb.cfg", and choose "notepad" from the option of available programs to "open with". You can list up to 8 device IDs but the app will only try to connect to the ones that are the same type, i.e., either 301 or 302. The .cfg file is supplied with random device ID's. Replace any or all with your device ID(s) and then save it. 3.) Run LL_USB2k.exe updated 6-20-12